{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":54,"n_cols":4,"rows_kept":54,"merged":[[36,0,36,3]],"flags":["formulas_cached_only"]}
["Event Name","Internal Name","Used in","Works?"]
["Initialisation_ref","C_EVENT_INIT_REF","(EventAgent.c - not sent)"]
["End_simu","C_EVENT_END_SIMU","(EventAgent.c - not sent)"]
["Component_state","C_EVENT_COMP_STATE","gw.cpp,sat.cpp,st.cpp,(EnvironmentAgent.c)","Yes"]
["Login_sent","C_EVENT_LOGIN_SENT","bloc_dvb_rcs_tal.cpp","Yes"]
["Login_received","C_EVENT_LOGIN_RECEIVED","bloc_dvb_rcs_ncc.cpp","Yes"]
["Login_response","C_EVENT_LOGIN_RESPONSE","bloc_dvb_rcs_ncc.cpp","Yes"]
["Login_complete","C_EVENT_LOGIN_COMPLETE","bloc_dvb_rcs_tal.cpp","Yes"]
["Connection_start","C_EVENT_CONNECTION_START","TestEnvironmentAgent.c"]
["Connection_stop","C_EVENT_CONNECTION_STOP","TestEnvironmentAgent.c"]
["BTP_discard_dynamic","C_EVENT_DISCARD_BTP_DYNAMIC","?"]
["C2P_connection_setup","C_EVENT_C2P_SETUP","?"]
["C2P_connection_setup_ack","C_EVENT_C2P_SETUP_ACK","?"]
["C2P_connection_mod","C_EVENT_C2P_MODIF","?"]
["C2P_connection_mod_ack","C_EVENT_C2P_MODIF_ACK","?"]
["C2P_connection_release","C_EVENT_C2P_RELEASE","?"]
["C2P_connection_release_ack","C_EVENT_C2P_RELEASE_ACK","?"]
[]
["GW Probe Name","Internal Name","Used in","Works?"]
["RBDC_requests_number","C_PROBE_GW_RBDC_REQUEST_NUMBER","lib_dama_ctrl_{yes,legacy}.cpp","Yes"]
["RBDC_requested_capacity","C_PROBE_GW_RBDC_REQUESTED_CAPACITY","lib_dama_ctrl_{yes,legacy}.cpp","Yes"]
["VBDC_requests_number","C_PROBE_GW_VBDC_REQUEST_NUMBER","lib_dama_ctrl_{yes,legacy}.cpp","Yes"]
["VBDC_requested_capacity","C_PROBE_GW_VBDC_REQUESTED_CAPACITY","lib_dama_ctrl_{yes,legacy}.cpp","Yes"]
["Uplink_fair_share","C_PROBE_GW_UPLINK_FAIR_SHARE","lib_dama_ctrl_legacy.cpp","No"]
["CRA_allocation","C_PROBE_GW_CRA_ALLOCATION","lib_dama_ctrl.cpp","Yes"]
["CRA_st_allocation","C_PROBE_GW_CRA_ST_ALLOCATION","lib_dama_ctrl.cpp","Yes"]
["RBDC_allocation","C_PROBE_GW_RBDC_ALLOCATION","lib_dama_ctrl_{yes,legacy}.cpp","Yes"]
["RBDC_st_allocation","C_PROBE_GW_RBDC_ST_ALLOCATION","lib_dama_ctrl.cpp","Yes"]
["RBDC_MAX_allocation","C_PROBE_GW_RBDC_MAX_ALLOCATION","lib_dama_ctrl.cpp","Yes"]
["RBDC_MAX_st_allocation","C_PROBE_GW_RBDC_MAX_ST_ALLOCATION","lib_dama_ctrl.cpp","Yes"]
["VBDC_allocation","C_PROBE_GW_VBDC_ALLOCATION","lib_dama_ctrl_{yes,legacy}.cpp","Yes"]
["FCA_allocation","C_PROBE_GW_FCA_ALLOCATION","lib_dama_ctrl_legacy.cpp","Yes"]
["Logged_ST_number","C_PROBE_GW_LOGGED_ST_NUMBER","lib_dama_ctrl.cpp","Yes"]
["BBFrame_sent_per_frame","C_PROBE_GW_BBFRAME_SENT_PER_FRAME","?","No"]
[]
["SAT Probe Name","Internal Name","Used in","Works?"]
["(No defined probes)"]
[]
["ST Probe Name","Internal Name","Used in","Works?"]
["Terminal_queue_size","C_PROBE_ST_TERMINAL_QUEUE_SIZE","bloc_dvb_rcs_tal.cpp","Yes"]
["Physical_outgoing_throughput","C_PROBE_ST_PHYSICAL_OUTGOING_THROUGHPUT","bloc_dvb_rcs_tal.cpp","Yes"]
["Real_incoming_throughput","C_PROBE_ST_REAL_INCOMING_THROUGHPUT","bloc_dvb_rcs_tal.cpp","Yes"]
["Real_outgoing_throughput","C_PROBE_ST_REAL_OUTGOING_THROUGHPUT","bloc_dvb_rcs_tal.cpp","Yes"]
["RBDC_request_size","C_PROBE_ST_RBDC_REQUEST_SIZE","bloc_dvb_rcs_tal.cpp","Yes"]
["VBDC_request_size","C_PROBE_ST_VBDC_REQUEST_SIZE","bloc_dvb_rcs_tal.cpp","Yes"]
["Allocation","C_PROBE_ST_ALLOCATION_SIZE","bloc_dvb_rcs_tal.cpp","Yes"]
["Unused_capacity","C_PROBE_ST_UNUSED_CAPACITY","bloc_dvb_rcs_tal.cpp","Yes"]
["CRA","C_PROBE_ST_CRA","bloc_dvb_rcs_tal.cpp","Yes"]
["Output_HDLB_rate","C_PROBE_ST_OUTPUT_HDLB_RATE","?","No"]
["Output_HDLB_packet_drops","C_PROBE_ST_OUTPUT_HDLB_DROPS","?","No"]
["Output_HDLB_backlog","C_PROBE_ST_OUTPUT_HDLB_BACKLOG","?","No"]
["BBFrames_droped_rate","C_PROBE_ST_BBFRAME_DROPED_RATE","bloc_dvb_rcs_tal.cpp","Yes"]
["Real_modcod","C_PROBE_ST_REAL_MODCOD","bloc_dvb_rcs_tal.cpp","Yes"]
["Received_modcod","C_PROBE_ST_USED_MODCOD","bloc_dvb_rcs_tal.cpp","Yes"]